**Nonwoven SPP Beard Cover**

**Basic Specifications**

Item code: PC61, PC62, PC63, PC64, PC65

Material: Nonwoven SPP 10gsm,

Colours available: white, blue, green, red, yellow

Size available: size 18”, 21”,

Style and design: with single elastic band or with double elastic band

Regular Pack: 100pcs/polybag, 1000pcs/ctn

**Description of Product**

Nonwoven SPP beard cover are made from breathable, comfortable and soft spun bonded polypropylene(SBPP) material which is commonly used in clean& hygiene rules, laboratory, clean room, hospital l& medical, food industry etc environment. It’s ideally for economical way to protect against non-hazardous dust particles and dirt in the work area.

**Features**

Made of non-woven breathable, soft, and comfortable material

Many colours available

Soft elastic for easy wearing

Wide range of application

**Quality Standard**

Production under ISO:9001:2008

CE category I

PPE Directive 89/686/EEC

FDA

REACH Regulation

**Suggested Application**

General hygiene and cleaning rules

Hospital and Medical

Food industry

Clean room

Household, Hotel etc

**Storage**

Please stock the goods in dry environment and avoid direct sunlight. Please don’t stock the goods in hot environment to temperature above 50℃ and humid above 80%. To keep away from high frequency equipment. Generally the shelf life is 6 years. We suggest you use products within 3 years.

**Instruction for use**

Please make sure the beard cover is well sewn and there is no hole and defect. The elastic band is in good quality. It’s not suitable to use this bouffant cap in dangerous working environment. Please don’t re-use. International care symbols: Do not wash Do not iron Do not machine dry

Do not dry clean Inflammable.

**How to select the appropriate products**

Firstly please make sure your purpose for use, then choose the right specification(size, quality, design etc) product which can bring you the most comforts and safety. If your working environment is hazardous and tough, we suggest you select higher grade Type 6 PB beard cover, safety hood cover etc to enhance protection performance.